Heater controller Memmert UM200

Requirements:

* Control the heaters via a solid state relais
* Display the actual temperature via 7-Segment displays
* Set the temperature using a potentiometer
* Power switch
* Communication via RS232 or RS485
* Controller: **PIC24FJ512GU410**